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EXPERIMENTAL OPERATING LIMITATIONS 

Exhibition           Group  2
(These limitations are derived from the national standards contained in FAA Order 8130.2G)
	REG. NO.
	MAKE:
	MODEL:
	SERIAL NO:

	54GT
	Yakovlev
	Yak-52
	833805


(1) No person may operate this aircraft for other than the purpose of exhibition, or to

participate in events, in accordance with 14 CFR § 21.193(d) or § 21.193(e). This aircraft must

be operated in accordance with all air traffic and general operating rules of 14 CFR part 91, all

limitations herein prescribed, and as described in the owner operator’s program letter. These

operating limitations are a part of FAA Form 8130-7, and are to be carried in the aircraft at all

times and be available to the pilot in command of the aircraft.

(2) No person may operate this aircraft unless FAA Form 8130-7 is displayed at the

cabin or cockpit entrance so that it is visible to passengers or flightcrew members, the word

“EXPERIMENTAL” is displayed in accordance with 14 CFR § 45.23, and the aircraft contains

the placards and markings required by 14 CFR § 91.9. The pilot in command of this aircraft must

advise passengers of the experimental nature of this aircraft and that it does not meet the

certification requirements of a standard certificated aircraft.

(3) The owner operator must submit an annual program letter to the geographically

responsible FSDO where the aircraft is based. All operations must be conducted in accordance

with these limitations and the program letter. A copy of the current program letter and any

amendments must be carried on board the aircraft any time that the aircraft is being operated.

The program letter must include the following information:

(a) The aircraft’s home base.

(b) The name of the person responsible for the operation and maintenance of the

aircraft.

(c) A list of events at which the aircraft will be exhibited (the list may be amended

as necessary).

(d) For Group 6 and Group 7 aircraft, the proficiency area may be depicted using a map or it may be described by geographic landmarks, airports, or aids to navigation.
(4) The pilot in command of this aircraft must hold an appropriate category and class

rating.

(9) During Phase I test flight operations, this aircraft is to be operated under VFR, day

only, and no person may be carried in this aircraft during flight unless that person is a required

crewmember. The local FSDO must approve if a person is essential for the test flight.

(10) During Phase I test flight operations, no person may flight test an aircraft except

over open water or sparsely populated areas having light air traffic.

(11) During Phase I test flight operations, this aircraft may only operate from [identify

name of airport(s)] until the requirements of 14 CFR § 91.319(b) have been met.) 
(12) During Phase I test flight operations, this aircraft must be operated for at least

_____hours with at least _____takeoffs and landings (to a full stop), and all operations must be

conducted in the geographic area described as follows:

(a) The size of the test flight area must be the minimum required to safely conduct

the anticipated maneuvers and tests.

(b) The area must be described by radius, and/or landmarks, or as depicted on an

attached chart.

(c) The minimum number of hours and minimum number of takeoffs and landings

should be based on the aircraft’s condition and records and the total time on the aircraft and its

engine(s).

(d) For aircraft other than newly manufactured or built, the number of hours

normally should normally be 10 and the minimum number of takeoffs and landings should be

five.

Note: For newly manufactured or newly built aircraft, Phase I test flight

limitations similar in scope to paragraph 4013b(3) and 4013b(4) of this

order will be added to these operating limitations.

(13) During Phase I test flight operations, following satisfactory completion of the

required number of flight hours in the flight test area, the pilot must certify in the records that the

aircraft has been shown to comply with 14 CFR § 91.319(b). Compliance must be recorded in

the aircraft records with the following, or a similarly worded, statement: “I certify that the

prescribed flight test hours have been completed and the aircraft is controllable throughout its

normal range of speeds and throughout all maneuvers to be executed, has no hazardous operating

characteristics or design features, and is safe for operation.”

(14) During Phase I test flight operations, aerobatic maneuvers intended to be

performed must be satisfactorily accomplished and recorded in the aircraft records during the

flight test period. In addition to the requirements of 14 CFR § 91.303, appropriate limitations

identifying the aerobatic maneuvers and conditions under which they may be performed shall be

included in the aircraft records.

(15) During Phase I test flight operations, if the aircraft will have removable externally

mounted equipment, it must be test flown in all configurations. An entry must be made in the

aircraft records indicating the configurations flight tested, unless the original manufacturer’s

flight test data for that equipment is included in the aircraft limitations.

(16) During Phase II operations, this aircraft is prohibited from flight with any

externally mounted equipment except in compliance with limitation (15) of this paragraph.

Note: The owner may place the aircraft back into Phase 1 for the sole

purpose of flight testing the added external equipment; in this case the owner must comply with limitation (15) requirements of this paragraph.
(17) During Phase II operations, this aircraft is prohibited from flight with any

externally mounted equipment unless the equipment is mounted in a manner that will prevent inflight jettison,

(18) During Phase II operations, except for takeoffs and landings (within class B, C, D,

or E surface airspace designated for the airport, or 5 NM, whichever is greater), this aircraft may

not be operated over densely populated, or congested areas except in compliance with

14 CFR § 91.119, or in an emergency situation. When exercising this authorization, the pilot in

command must avoid densely populated areas and congested areas whenever possible.

(21) During Phase II operations, no person may be carried in this aircraft during the

exhibition of the aircraft’s flight capabilities, performance, or unusual characteristics at airshows,

or for motion picture, television, or similar productions, unless essential for the purpose of the

flight. Persons may be carried during flights to and from any event or during proficiency/currency flying, limited to the design seating capacity of the aircraft and subject to

the regulatory prohibition on compensation. The pilot in command of this aircraft must advise

the passenger of the experimental nature of this aircraft and that it does not meet the certification

requirements of a standard certificated aircraft.

(24) During Phase II operations, aerobatic maneuvers that were not satisfactorily

accomplished and recorded during the Phase I flight test time period may not be performed.

Note: The owner may place the aircraft back into Phase 1 for the sole purpose of

adding additional aerobatic maneuvers to the aircraft authorized maneuvers. In

this case, the owner must comply with limitation (13) requirements of this

paragraph.

(26) This aircraft must not be used for glider towing, banner towing, or

recreational/sport parachute jumping.

(27) During Phase II operations, night and/or instrument flight is approved, provided

the aircraft is equipped as described in 14 CFR § 91.205. Instruments and equipment installed for

night and/or instrument flight must be inspected and maintained in accordance with the

applicable requirements of 14 CFR part 91. All maintenance or inspection of this equipment

must be recorded in the aircraft maintenance records.

(28) Equipment installed to meet regulatory requirements must be inspected and

maintained in accordance with the applicable requirements of 14 CFR part 91. Any maintenance

or inspection of this equipment must be recorded in the aircraft maintenance records.

(29) All large airplanes, turbojet airplanes, turbopropeller-powered multiengine

airplanes, or turbine-powered rotorcraft must be maintained in with accordance an FAA

approved inspection program meeting the scope and content as described in 14 CFR § 91.409(f).

Completion of these inspections must be recorded in the aircraft maintenance records.

(30) Inspections for all large airplanes, turbojet airplanes, turbopropeller-powered

multiengine airplanes, and turbine-powered rotorcraft must be recorded in the aircraft

maintenance records showing the following, or a similarly worded, statement: “I certify that this

aircraft has been inspected on [insert date] in accordance with the scope and detail of [identify

applicable inspection program] and found to be in a condition for safe operation.”

(31) No person may operate aircraft other than those described in limitations (29) and

(30) of this paragraph unless within the preceding 12 calendar months it has had a condition

inspection performed in accordance with the scope and detail of 14 CFR part 43, appendix D, or

other FAA-approved programs, and was found to be in a condition for safe operation. This

inspection will be recorded in the aircraft maintenance records.

(32) Condition inspections for aircraft other than those described in limitations (29)

and (30) of this paragraph must be recorded in the aircraft maintenance records showing the

f[insert date] in accordance with the scope and detail of 14 CFR part 43, appendix D, and found to be in a condition for safe operation.” The entry will include the aircraft’s total time-in-service

and the name, signature, certificate number, and type of certificate held by the person performing

the inspection.

(33) Only FAA-certificated mechanics with appropriate ratings as authorized by

14 CFR § 43.3 may perform inspections required by these operating limitations.

(34) The cognizant FSDO must be notified, and its response received in writing, prior

to flying this aircraft after incorporation of a major change as defined by 14 CFR § 21.93 in

order to determine whether new operating limitations will be required. The FSDO response

should be entered in the aircraft's records and a copy sent the FAA Aircraft Registration Branch,

AFS-750, P.O. Box 25504, Oklahoma City, Oklahoma 73125 for recording in the aircraft’s

permanent records.

(36) The special airworthiness certificate and attached operating limitations for this

aircraft have no expiration date.

(37) When an aircraft’s home base is changed or there is a transfer of ownership, the

new owner/operator will take any or all of the following actions within 30 days:

(a) Submit a new program letter to the geographically responsible FSDO.

(b) If an approved inspection program is specified in these operating limitations,

submit a copy to the geographically responsible FSDO. The gaining FSDO will not change the

previously approved program unless it can be substantiated that the previously approved program

no longer meets FAA requirements.

(c) The gaining FSDO will not require the aircraft’s airworthiness certificate or

operating limitations to be reissued, unless the aircraft requires Phase I test flight operations.

(38) This aircraft does not meet the requirements of the applicable, comprehensive,

and detailed airworthiness code as provided by Annex 8 to the Convention on International Civil

Aviation. The owner/operator of this aircraft must obtain written permission from another

country’s CAA before operating this aircraft in or over that country. That written permission

must be carried aboard the aircraft together with the U.S. airworthiness certificate and, upon

request, be made available to an ASI or the CAA in the country of operation. 

(39) Application must be made to the geographically responsible FSDO for any

revision to these operating limitations.

(41) The special airworthiness certificate and attached operating limitations for this

aircraft have no expiration date. New proficiency areas must be described for Group 6 or 7

aircraft.

(42) FAA approval of maintenance and inspection interval extensions requires that the

owner operator submit documentation and data justifying the extension to the local FSDO for

elevation for concurrence.

(43) Approval of life limit extensions may be approved by the FAA only if the original

manufacturer approves and provides documentation supporting the extension. In the case that

original manufacturer data is not available, an appropriately qualified DER may provide data to

substantiate life limit extension, but the FAA must concur with the results of the data.

(44) Aircraft originally incorporating fatigue life recording systems must maintain the

system and comply with the original manufacturer fatigue limits. If the fatigue life system is

removed, or is inoperative, the aircraft cannot be operated in any group other than Group 6.

Joseph R. Broker

ASI
Date Issued: April 21, 2011
ACKNOWLEDGMENT OF SPECIAL

OPERATING LIMITATIONS

TO WHOM IT MAY CONCERN:
I certify that I have read and understand the Special Operating Limitations which are a part of the Special Airworthiness Certificate, FAA Form 8130-7, issued _01/03/2010.

This Airworthiness Certificate is issued for aircraft make  Six Chuter model SR5, serial number 99-2259-SR5,

and registration number _N94330.

______________                               _
_01/03/2010_
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